Patch-ID# 109897-20
Keywords: security usb usba scsa2usb audio hubd hotplug-aware usb
Synopsis: SunOS 5.8_x86: USB and Audio Framework patch
Date: Aug/24/2004


Install Requirements: Reconfigure immediately after patch is installed                      
                      
Solaris Release: 8_x86

SunOS Release: 5.8_x86

Unbundled Product: 

Unbundled Release: 

Xref: This patch available for sparc as patch 109896

Topic: SunOS 5.8_x86: USB and Audio Framework patch
	NOTE:	Refer to Special Install Instructions section for
		IMPORTANT specific information on this patch.

Relevant Architectures: i386

BugId's fixed with this patch: 4042931 4178572 4179082 4204158 4207634 4257491 4271687 4278766 4282084 4282600 4284408 4284481 4288456 4290035 4290038 4290048 4292644 4295049 4295084 4297451 4297991 4298047 4299321 4299711 4300133 4300497 4301110 4302343 4302435 4303153 4303369 4303371 4304019 4304060 4304250 4304253 4304383 4304911 4304968 4305434 4305436 4305437 4305467 4305645 4305649 4305819 4306676 4307085 4307415 4307418 4307542 4308510 4308511 4309075 4309328 4309368 4309499 4309566 4309916 4311023 4312163 4312381 4313650 4314164 4314166 4315368 4317503 4317522 4317527 4317528 4317916 4318194 4318604 4320410 4321542 4323024 4326037 4326139 4326143 4328521 4328542 4328590 4329325 4329560 4329687 4330021 4331700 4331710 4331762 4331764 4331769 4331858 4332033 4332613 4332707 4333033 4333036 4333039 4333879 4336235 4336592 4337149 4337561 4337816 4338525 4338614 4339292 4339729 4341714 4341839 4342024 4342426 4342488 4343230 4343443 4343762 4344107 4344121 4344122 4346254 4346837 4346963 4347288 4348120 4348124 4349013 4349282 4349339 4350113 4350570 4350901 4351164 4351268 4351426 4351563 4351568 4351707 4352002 4352101 4352320 4352931 4353816 4353820 4357035 4357915 4359440 4359658 4359875 4361715 4361718 4361719 4362924 4363252 4363632 4363966 4364027 4364427 4364534 4364575 4364748 4364911 4365137 4365848 4366366 4366395 4366523 4366651 4366874 4367554 4367841 4368474 4369136 4369166 4369411 4369968 4370685 4370687 4370697 4372725 4373367 4374495 4374566 4374608 4374609 4374774 4374933 4375698 4375740 4375879 4375900 4376086 4376175 4377947 4378118 4378262 4378867 4379087 4380154 4380598 4381028 4382906 4384717 4384776 4384791 4385510 4387466 4387888 4388157 4388286 4388586 4388935 4391440 4391912 4392605 4393088 4393114 4393350 4393591 4393819 4393967 4398235 4400665 4402359 4402755 4404373 4404398 4404559 4408726 4409022 4410980 4411451 4412128 4412479 4415430 4416071 4416096 4417060 4417092 4417298 4418923 4420873 4423037 4423482 4423523 4426338 4433464 4437766 4440473 4442483 4447095 4449060 4449744 4451857 4451865 4452562 4457209 4463426 4464517 4465102 4469049 4478723 4490191 4490193 4507103 4587859 4655789 4660099 4663786 4670245 4701098 4714088 4735539 4750685 4757590 4765718 4776340 4785916 4786786 4790888 4800123 4801046 4804860 4812935 4834143 4836298 4838235 4841489 4852863 4854629 4964108 5028398 5070166

Changes incorporated in this version: 5070166

Patches accumulated and obsoleted by this patch: 109315-03 109342-01 109875-01 111529-03 113422-01

Patches which conflict with this patch: 

Patches required with this patch: 108529-29 or greater 109884-01 or greater 110610-04 or greater

Obsoleted by: 

Files included with this patch: 

/etc/driver_aliases
/etc/format.dat
/etc/init.d/initusb
/etc/name_to_major
/etc/rcS.d/S49initusb
/kernel/drv/hid
/kernel/drv/hubd
/kernel/drv/scsa2usb
/kernel/drv/uhci
/kernel/drv/usb_mid
/kernel/drv/usbprn
/kernel/misc/usba
/kernel/strmod/usbkbm
/kernel/strmod/usbms
/usr/include/sys/ac97.h
/usr/include/sys/audio.h
/usr/include/sys/audio/am_src1.h
/usr/include/sys/audio/audio_apm.h
/usr/include/sys/audio/audio_mixer.h
/usr/include/sys/audio/audio_src.h
/usr/include/sys/audio/audio_support.h
/usr/include/sys/audio/audio_trace.h
/usr/include/sys/audio_impl.h
/usr/include/sys/audiodebug.h
/usr/include/sys/audioio.h
/usr/include/sys/g711.h
/usr/include/sys/mixer.h
/usr/include/sys/mixer_impl.h
/usr/include/sys/usb/clients/audio/usb_audio.h (deleted)
/usr/include/sys/usb/clients/mass_storage/usb_bulkonly.h
/usr/include/sys/usb/clients/printer/usb_printer.h
/usr/include/sys/usb/usba.h
/usr/include/sys/usb/usbai.h
/usr/kernel/drv/usb_ac
/usr/kernel/drv/usb_ac.conf
/usr/kernel/drv/usb_as
/usr/kernel/misc/amsrc1
/usr/kernel/misc/audiosup
/usr/kernel/misc/audiosup.conf
/usr/kernel/misc/diaudio
/usr/kernel/misc/mixer
/usr/kernel/misc/mixer.conf
/usr/lib/adb/am_ad_info
/usr/lib/adb/am_ch_private
/usr/lib/adb/audio_apm_info
/usr/lib/adb/audio_ch
/usr/lib/adb/audio_channel
/usr/lib/adb/audio_device
/usr/lib/adb/audio_info
/usr/lib/adb/audio_prinfo
/usr/lib/adb/audio_state
/usr/lib/adb/audiotrace
/usr/lib/adb/audiotrace.nxt
/usr/lib/adb/hubd
/usr/lib/adb/ohci_ed
/usr/lib/adb/ohci_hcca
/usr/lib/adb/ohci_pipe_private
/usr/lib/adb/ohci_polled
/usr/lib/adb/ohci_regs
/usr/lib/adb/ohci_root_hub
/usr/lib/adb/ohci_state
/usr/lib/adb/ohci_td
/usr/lib/adb/ohci_trans_wrapper
/usr/lib/adb/ohci_usb_dev
/usr/lib/adb/openhci_state		(deleted file)
/usr/lib/adb/scsa2usb_cmd
/usr/lib/adb/scsa2usb_state
/usr/lib/adb/src1_data
/usr/lib/adb/src1_info
/usr/lib/adb/uhci_pipe_private
/usr/lib/adb/uhci_polled
/usr/lib/adb/uhci_qh
/usr/lib/adb/uhci_state
/usr/lib/adb/uhci_td
/usr/lib/adb/uhci_trans_wrapper
/usr/lib/adb/usb_ac_plumbed
/usr/lib/adb/usb_ac_power
/usr/lib/adb/usb_ac_state
/usr/lib/adb/usb_ac_streams_info
/usr/lib/adb/usb_ac_to_as_req
/usr/lib/adb/usb_as_alt_descr
/usr/lib/adb/usb_as_power
/usr/lib/adb/usb_as_state
/usr/lib/adb/usb_audio_formats
/usr/lib/adb/usb_device
/usr/lib/adb/usb_isoc_pkt_descr
/usr/lib/adb/usb_isoc_request
/usr/lib/adb/usb_pipe_policy
/usr/lib/adb/usb_streams_registration
/usr/lib/adb/usbkbm_state
/usr/lib/adb/usbprn_def_arg
/usr/lib/adb/usbprn_power
/usr/lib/adb/usbprn_ps
/usr/lib/adb/usbprn_reset_arg
/usr/lib/adb/usbprn_state
/usr/lib/mdb/kvm/usba.so

Problem Description:

5070166 has incorrect dependency on 108528-20
 
(from 109897-19)
 
5028398 System panics on exit from OS, after arriving at the prom-level
 
(from 109897-18)
 
4964108 The postpatch script for patch # 109897-17 fails to load in a diskless client
 
(from 109897-17)
 
4801046 suspend ohci controller during CPR suspend if usb keyboard is not connected
 
(from 109897-16)
 
4852863 USB audio does not correctly register full duplex devices with mixer
4854629 mouse rev 105 does not respond to first get hid descriptor request
4812935 add support for ELO touch screen (Heidelberg)
4785916 ugen doesn't protect from bogus control message lengths
4786786 ugen returns EIO on bulk write out endpoints for a USB Canon Scanner N670U
4757590 minor lint fix and cleanup
4838235 ugen: poll on devstat doesn't block
4834143 ugen must validate wLength to buf b_bcount
4836298 non-exclusive endpoint opens not allowed
4841489 ugen: incorrect buffer full status on disconnect
 
(from 109897-15)
 
4800123 Netra AC200 USB audio does not work reliably.
4507103 prtconf hangs during hotplugging
4804860 usb_as:  base sample rate should be checked before reducing sr list
 
(from 109897-14)
 
4776340 ON support for new platforms
4452562 assert failure in hubd_determine_port_status
4655789 key up events lost when keys held down on multiple keyboards at once
4663786 system panics when the usb keyboard and mouse are hot plugged
4750685 MDB support for USB debug buffers needed for fiesta platform
4765718 Need to press STOP key twice for L1-A on enchilada and taco systems
4790888 Audio mixer panic while running application stress tests.
 
(from 109897-13)
 
4714088 cannot control volume with patch 109896-08 and 109748-03 installed in compat mod
 
(from 109897-12)
 
4587859 I_STR ioctl payloads are improperly validated
 
(from 109897-11)
 
4464517 RED State Exception on SB100/SB1000 while booting with Addonics USB DVD
 
(from 109897-10)
 
4670245 Audio quality on sunblade 100 is not as good as sunblade 1000,U10, etc.
4701098 play.samples element in audio_info struct doesn't update with patch 109896-07
4660099 warlock looking in /usr/include for sparc
 
(from 109897-09)
 
4490193 USB performance against Hagiwara devices isn't great on INTELS only
 
(from 109897-08)
 
4490191 usb nexus should not call pm idle when it is not powering off
 
(from 109897-07)
 
4463426 mixer needs to check the hardware sample rate before enabling mixer mode
4469049 frame buffer power management activities make CPU busy
4478723 hubd should not call pm idle when it is not powering off
 
(from 109897-06)
 
	This patch revision was generated to accumulate and obsolete
        the feature changes introduced in point patch 111529-03.
 
(from 109897-05)
 
4416071 Disable all the interrupts before calling ddi_get_iblock_cookie()
 
(from 109897-04)
 
4300133 Isoc support in ohci
4178572 Isochronous support must be added to the USB framework
4315368 Add Isochronous Support to UHCI
4042931 ohci should support for frame number overflow interrupt
4338614 usb_pipe_open returns "USB_NO_BANDWIDTH" for wMaxPacketSize=0
4204158 Interrupt polling for less than 3ms is not accurate
4353820 add cdr/cd-rw support to scsa2usb
4326037 add usbprn x86 support
4352931 panic in uhci - machine left idle overnight (Intel Only)
4359440 Grover with 128MB dimm  paniced with usb devices during boot time.
4349339 Large postscript or ascii files are not printed completely on usb printer(x86)
4307542 uhci needs to return no. of bytes successfully sent in bulk xfer timeout
4362924 USB stops working; apparent deadlock
4363252 hotplug_thread hang at ndi_event_add_callback & i_ndi_block_device_tree_changes
4364427 Hubd should not raise power for a device that is in detach
4366874 System panics due to dead lock condition
4359875 'phantom' usb_device structs left in list on hot unplug
4365848 Misuse of dma/memory handles in uhciutil.c
4305434 driver needs to put device in low power at detach time
4305436 driver needs to put device in low power at detach time
4331710 ohci is broken on x86 platform
4357035 put device in low power mode at detach time.
4357915 "Device disk1 failed to power up" for USB FlashGate device
4364575 check first if remotewakeup is supported before invoking it
4364748 scsa2usb needs enable and disable remote wakeup during attach and detach
4366523 remove assert after usbprn_clear_feature()
4313650 UHCI should return number of bytes received in case of "OVER RUN" condition
4328590 Data toggle handling needs change.
4350570 usb_prn adb macro should not use y
4359658 verify parental notification duties for hubd and usb_mid
4365137 hubd should cleanly maintain port states
4343762 Rename adb macro openhci_state to ohci_state
4295084 Change minor name format in hid
4333879 Correct typo in usb_printer.h
4346254 checking interrupt context needs to be done with servicing_interrupt()
4380154 usb warlock files are inconsistent in Solaris 8 update gate
 
(from 109897-03)
 
4369166 I-DEAS F1+Mouse does not work on USB kbds
 
(from 109897-02)
 
4346963 ohci_handle_ue shouldn't call debug_enter
4350113 ohci root hub timeout is not restarted under allocb failure
4352101 UHCI_INTR_MASK macro value is wrong
4349282 prtconf hung when a protype Lex Mark printer connected at Plugfest
4314164 Error message "connecting device on port 1 failed" displayed when no devices ar
4308510 panic in uhci mutex_enter: uhci_sendup_td_message
4308511 panic in uhci mutex_enter: uhci_handle_intr_td_errors
4349013 zip driver won't suspend, even after drive is removed from system
4350901 scsa2usb_bulkin reset called after scsa2usb_bulkout reset
4351707 Stop issuing GET_MAX_LUN to USB zip drives
4347288 print a message when a device is in use and a user 'hot removes' it
4344122 usb_get_string_descriptor() can panic the system
4351268 string descriptors not being properly filled in
4351426 usb_dprintf0 adds an extra newline to the message on the console
4344107 panic when usba_clear_print_buf is called from kadb in non-debug kernel
 
(from 109897-01)
 
	This patch revision was generated to accumulate and obsolete
	the feature changes introduced in point patch 109315-03.
 
4179082 Remove RIO specific code from ohci driver after RIO pass2
4207634 usb packages : remove "pci108e,1103" entry from /etc/driver_aliases
4278766 assertion failed: ph->p_sync_result.p_done == 0 with usb_bobo
4282084 Need a mechanism to specify different timeouts for each command sent out on USB
4284481 uhci_cleanup refers to freed memory, panics DEBUG kernel
4297991 Beep goes non-stop  during console kbd/ms hotplug
4305437 driver needs to put device in low power at detach time
4312163 cleanup minor nits in usb files
4314166 usba: redundant check in usb_pipe_sync_close/usb_pipe_release on valid pipe
4323024 Extra device node created for Epson printer.
4329325 System panics on x86 with the usbprn driver on on81 gate
4329560 warlock.usb fails with errors on on81
4330021 GET_MAX_LUN bRequest and bmRequestType are in reverse order
4331700 usb_get_string_descriptor() panics in scsa2usb as len is less
4332033 usba/parser.c: none of the functions check for "ret_buf_len"
4332613 cybex hid device needs workaround to support multiple report id
4332707 need a function to figure out different alternate interfaces.
4336592 Castlewood ORB 2.2 GB drive does not work on x86
4337149 ohci: NULL pointer dereference during cpr on new platform
4337561 enable attaching Imation's USB LS-120 drive to scsa2usb
4338525 running label (under format) on zip100 returns error message
4339292 possible TRAP in ohci.c
4341839 Remove RIO1 specific code in ohci driver
4328542 hubd set feature port enable need to distinguish between root hub vs regular hub
4307085 USB printer support required on Solaris
4309566 64 bytes data loss problem with Lexmark Optra 310 when paper out
4312381 ohci should return whatever data received under data overrun condition
4317503 usb_mid: always enable PM
4317522 usba: eliminate assert on prop function's return value
4317527 hub driver needs to raise power level at attach time, lower at detach
4317528 usb_mid driver needs to raise power level at attach time, lower at detach
4257491 ohci cannot do 8k transfer per TD
4284408 usb_mid/hid need some clean up with respect to states
4288456 assertion failed: rval == USB_SUCCESS, file: ../../common/io/usb/usba/hubdi.c,
4290035 Workaround needed for Microsoft IntelliMouse & keyboard
4290038 root hub interrupt events must be emulated correctly
4290048 hubd may need to handle disconnect/reconnect
4297451 USB Power Management is incorrectly disabled on RIO Pass 2
4298047 Hangs on booting; also prtconf hangs
4299321 assertion in usb_mid regards mi_dev_state
4299711 assert caught while doing USB suspend/resume on PPX with rio 2.0
4301110 Add kadb macros to UHCI
4302435 USB_SHORT_XFER_OK instead of USB_FLAGS_SHORT_XFER_OK in usbai.h
4303153 ch11 tests fail with timeouts on UHCI
4303371 ohci code cleanup
4304019 get_max_lun request to hagiwara's flash gate device confuses it w/ ohci
4304060 ohci data structures and adb macros must have driver prefixes
4304250 Data under run case is not handled properly
4304253 Bulk Performance on UHCi is not good
4304383 cleanup usb_mid event posting mechanism
4304968 usb_pipe_close doesn't check if the pipe handle is NULL.
4305467 Bulk devices starve for the execution
4305645 ohci should return number of bytes transmitted when send command fails
4309916 hub enumeration fails on UHCI
4303369 Data toggle mismatch across pipe open/close and pipe reset between host & device
4305649 ohci TD  fields and definitions names must be changed appropriately
4305819 ohci incorrectly reports 4096 for min PCI clock
4306676 usba_impl.h should not be included in client drivers
4309328 memory leak in scsa2usb_bulk_only_transport()
4309368 usba_hcdi_soft_intr() uses PRINT_MASK_HCDI which is wrong
4311023 usba_destroy_pipe_handle() must wait for sync cmds to complete
4320410 /devices entries for USB devices have wrong permissions
4336235 Hid needs to power manage the new mouse
4342024 usb pipe policy changes need to be rev'ed
4342426 memory leak in usba_async_request_raise_power()
4342488 Move debug_enter code under ifdef DEBUG
4343443 for all usb devices check if they are bound to a driver; and report error if not
4341714 warn user that no driver has been found
4344121 memory leak in hid_default_pipe_exception_callback()
4337816 hubd panic during hotplug with hid tests
4343230 memory leak in usbms_wput()
 
(from 109315-03)
 
4336235 Hid needs to power manage the new mouse
4342024 usb pipe policy changes need to be rev'ed
4342426 memory leak in usba_async_request_raise_power()
4342488 Move debug_enter code under ifdef DEBUG
4343443 for all usb devices check if they are bound to a driver; and report error if not
4341714 warn user that no driver has been found
4344121 memory leak in hid_default_pipe_exception_callback()
4337816 hubd panic during hotplug with hid tests
4343230 memory leak in usbms_wput()
 
(from 109315-02)
 
4179082 Remove RIO specific code from ohci driver after RIO pass2
4207634 usb packages : remove "pci108e,1103" entry from /etc/driver_aliases
4278766 assertion failed: ph->p_sync_result.p_done == 0 with usb_bobo
4282084 Need a mechanism to specify different timeouts for each command sent out on USB
4284481 uhci_cleanup refers to freed memory, panics DEBUG kernel
4297991 Beep goes non-stop  during console kbd/ms hotplug
4305437 driver needs to put device in low power at detach time
4312163 cleanup minor nits in usb files
4314166 usba: redundant check in usb_pipe_sync_close/usb_pipe_release on valid pipe
4323024 Extra device node created for Epson printer.
4329325 System panics on x86 with the usbprn driver
4329560 warlock.usb fails with errors
4330021 GET_MAX_LUN bRequest and bmRequestType are in reverse order
4331700 usb_get_string_descriptor() panics in scsa2usb as len is less
4332033 usba/parser.c: none of the functions check for "ret_buf_len"
4332613 cybex hid device needs workaround to support multiple report id
4332707 need a function to figure out different alternate interfaces.
4336592 Castlewood ORB 2.2 GB drive does not work on x86
4337149 ohci: NULL pointer dereference during cpr on new platform
4337561 enable attaching Imation's USB LS-120 drive to scsa2usb
4338525 running label (under format) on zip100 returns error message
4339292 possible TRAP in ohci.c
4341839 Remove RIO1 specific code in ohci driver
4328542 hubd set feature port enable need to distinguish between root hub vs regular hub
 
(from 109315-01)
 
4307085 USB printer support required on Solaris
4309566 64 bytes data loss problem with Lexmark Optra 310 when paper out
4312381 ohci should return whatever data received under data overrun condition
4317503 usb_mid: always enable PM
4317522 usba: eliminate assert on prop function's return value
4317527 hub driver needs to raise power level at attach time, lower at detach
4317528 usb_mid driver needs to raise power level at attach time, lower at detach
4257491 ohci cannot do 8k transfer per TD
4284408 usb_mid/hid need some clean up with respect to states
4288456 assertion failed: rval == USB_SUCCESS, file: ../../common/io/usb/usba/hubdi.c,
4290035 Workaround needed for Microsoft IntelliMouse & keyboard
4290038 root hub interrupt events must be emulated correctly
4290048 hubd may need to handle disconnect/reconnect
4297451 USB Power Management is incorrectly disabled on RIO Pass 2
4298047 Hangs on booting; also prtconf hangs
4299321 assertion in usb_mid regards mi_dev_state
4299711 assert caught while doing USB suspend/resume on PPX with rio 2.0
4301110 Add kadb macros to UHCI
4302435 USB_SHORT_XFER_OK instead of USB_FLAGS_SHORT_XFER_OK in usbai.h
4303153 ch11 tests fail with timeouts on UHCI
4303371 ohci code cleanup
4304019 get_max_lun request to hagiwara's flash gate device confuses it w/ ohci
4304060 ohci data structures and adb macros must have driver prefixes
4304250 Data under run case is not handled properly
4304253 Bulk Performance on UHCi is not good
4304383 cleanup usb_mid event posting mechanism
4304968 usb_pipe_close doesn't check if the pipe handle is NULL.
4305467 Bulk devices starve for the execution
4305645 ohci should return number of bytes transmitted when send command fails
4309916 hub enumeration fails on UHCI
4303369 Data toggle mismatch across pipe open/close and pipe reset between host & device
4305649 ohci TD  fields and definitions names must be changed appropriately
4305819 ohci incorrectly reports 4096 for min PCI clock
4306676 usba_impl.h should not be included in client drivers
4309328 memory leak in scsa2usb_bulk_only_transport()
4309368 usba_hcdi_soft_intr() uses PRINT_MASK_HCDI which is wrong
4311023 usba_destroy_pipe_handle() must wait for sync cmds to complete
4320410 /devices entries for USB devices have wrong permissions
 
(from 109875-01)
 
	This patch revision was generated to accumulate and obsolete
	the feature changes introduced in point patch 109342-01.
 
4271687 AC-97 compliant audio driver is needed for new platform using Acer South Bridge.
4304911 Switching modes while recording panics with a null pointer dereference
4307415 audio mixer panics when audio driver doesn't support monitor feature
4329687 Audio packages need depend files installed in packages
 
(from 109342-01)
 
4271687 AC-97 compliant audio driver is needed for new platform using Acer South Bridge.
4304911 Switching modes while recording panics with a null pointer dereference
4329687 Audio packages need depend files installed in packages
 
(from 111529-03)
 
4449060 usb_as_serialize_access need to check on current thread
4437766 grover panics with a deadbeef in usb_ac
4442483 problem in pm with USB audio drivers
4449744 ohci panic during callback
4426338 scsa2usb: hang while opening default pipe
4451865 Larger timeout for SOF interrupt event
4423523 Telex microphone fails to enumerate when connected through a hub
4402359 loud hiss sounds from excalibur during audio testing
4457209 audiocs driver has audio quality problems with record on SunVTS
4351568 sample count sometimes goes backwards when FLUSHW ioctl is used
4433464 ultra1 panics with vmem_xalloc(): size == 0
4440473 turn signals back on for mode changes
4447095 New southbridge hardware also requires a software workaround for audio
4451857 mixer hangs on close.
 
(from 111529-02)
 
4465102 S8 U6 Build 2: WARNING: mod_load: cannot load module 'usb_ac' and 'usb_as'
 
(from 111529-01)
 
4346837 USB audio support is needed on Solaris
4282600 ohci should recover gracefully under no SOF condition
4361715 Improper interrupt/bulk data toggle handling
4361718 ohci: enhance interrupt pipe polling for one time polling
4361719 uhci: enhance interrupt pipe polling for one time polling
4366395 ohci misuses dma/memory handles
4367554 scsa2usb panic during hotplugging with multi lun storage device
4367841 usbprn returns two length bytes in ECPPIOC_GETDEVID
4368474 Interrupt Data toggle handling needs change.
4369136 Build uhci on sparc so we can warlock it
4369411 ohci hits panic due to null pointer deference in ohci_hcdi_pipe_close
4369968 remove the dead code in uhci_hcdi_clinet_init, _fini, pipe open, pipe close ent
4370685 ohci must print more verbose message for any error
4370687 Argument for usb_hcdi_bulk_transfer_size() must be usb_device instead of dip
4370697 Add makefile to build ohci on X86
4373367 usbprn errno values to be consistent with ecpp errno vales.
4374608 ohci: send dummy message block under zero bytes IN data transfer condition
4374609 uhci: send dummy message block under zero bytes IN data transfer condition
4375740 usba: pipe is not opened exclusively
4379087 usba need not calculate strlen in usb_vprintf
4382906 enhance usb_unpack_LE_data functions to parse big and complex descriptors
4385510 Enumeration of scm media card hang in usba_handle_device_remote_wakeup
4388157 usb printer doesn't print complete file under paper out condition
4388935 ohci_td adb macro dumps information incorrectly
4392605 Race condition between UHCI hardware and UHCI driver
4398235 kernel heap corruption in ohci if more requests are queued for isoc
4409022 During Solaris 9 build 30 install "WARNING:usba:Onlining ...device failed"
4410980 panic with BAD  TRAP type 31 in ohci due to NULL pointer dereference
4412479 ohci cleanup in pipe close, pipe reset and other places
4417060 Change USBA_TASKQ_N_THREADS and USBA_TASKQ_MAXALLOC default values in usba
4420873 ohci checks wrong bits while saving/restoring data toggle information
4423037 ohci: memory leak during usb audio reocrd
4374774 audio driver reimplementation
4292644 audio volume changes in an inconsistent fashion
4295049 deadlock using AUDIO_MIXERCTL_SET_CHINFO ioctl
4300497 The audio mixer blows an assertion when switching modes with showmetv playing
4302343 The play waiting flag remains set after switching to mixer mode
4307415 audio mixer panics when audio driver doesn't support monitor feature
4307418 audio mixer doesn't handle balance correctly in compat mode with mono
4309075 New audio driver and modules use deprecated property interfaces
4309499 am_send_audio() should reject 0 sized samples
4317916 mixer: remove record and play restriction
4318194 new audio hearders need the file guards updated
4318604 Separate sample rate conversion code from the audio mixer
4321542 wrong spelling on error message return by mixerctl
4326139 move new audio modules to common source in preparation for x86 port
4326143 add new adb and forthdebug macros for audio modules and drivers
4328521 support the new audio driver architecture on x86 Solaris
4331762 audio mixer feedback mechanism for hardware changes is broken
4331764 fix audio mixer interface so a pointer to a lock is no longer passed
4331769 audio interfaces should use an opaque handle
4331858 audio mixer sample rate conversion routine shouldn't use apm_info structure
4333033 mixer:  non-blocking callbacks cannot be implemented with USB audio driver
4333036 mixer:  AUDIO_PRECISION_8 should not be a requirement for play combinations
4333039 mixer: error messages should include audio driver and instance number
4339729 driver & mixer configuration thru properties needs rework
4348120 audiosup: replace use of ddi_soft_state by linked list
4348124 audiosup: provide audio_sup_getinfo interface
4351164 audio adb macros broken
4351563 play.sample resolution reduced greatly in Solaris 8
4352002 am_open doesn't always call ad_teardown when it should
4352320 panic caused by multiple audio channels with mixer off
4353816 assertion failure/panic: stpptr->am_active_ioctls == 0
4363632 audio driver architecture needs to support drivers that use special open/close
4363966 noise is generated when audio mixer is paused and mode is switched
4364027 The audiots set_format() routine always returns AUDIO_SUCCESS
4364534 audiosup: audio_sup_get_qptr_instance
4364911 am_close code is racy
4366366 System panics while resuming from a checkpoint
4366651 Error freeing access handles in audio_4231_eb2dma.c
4372725 warlock mixer + audiosup + amsrc1 + audiots/cs
4374495 The audiocs and audiots audio drivers should use audio_sup_log
4374566 audio source code directory reorganization
4374933 audio_sup_get_qptr_data() needs to check for a null pointer
4375698 reimplemented audio mixer panics on MP machines
4375879 reimplemented audio mixer breaks SunVTS with audiots driver
4375900 make AUDIO_MIXER_GET_SAMPLE_RATES ioctl() available for audioctl channels
4376086 audio is distorted when the mode is switched couple of times
4376175 reimplemented audio mixer panics in Close_no_drain test
4377947 panic in mixer module due to NULL pointer dereference
4378118 Play_EOF test fails with reimplemented audio mixer driver
4378262 most audio header files need disclaimer
4378867 panic in audio mixer module with assertion fail
4380598 assertion failed in am_main while playing with audioplay and changing modes
4381028 record sample count does not increment in mixer mode
4384717 audiocs and audiots drivers cause audio mixer to deadlock
4384776 The audiocs driver has many large functions that need to be simplified
4384791 The audiocs driver's power management routines need cleanup
4387466 The audiocs macros REG_SELECT and DDI_PUT8 should be changed to functions
4387888 Provide a method to more easily restart audio
4388286 assertion failed:  !am_task_is_frozen(stpptr->am_taskq) in am_main.c
4388586 SUNW,Sun-Blade-1000 panics with BAD TRAP: type=31 in am_get_audio_trad_mixer
4391440 assertion failed: data->adata_optr == data->adata_orig,file: am_ad.c, line: 2657
4391912 SUNW,Sun-Blade-1000 panics with BAD TRAP while audioplay and switching modes
4393088 SUNW,Sun-Blade-1000 panics with deadbeef corruption
4393114 audioplay hangs while playing sample.au and switching modes on grover and USB
4393350 SUNW,Sun-Blade-100 panics with a bad trap type:30
4393591 audioplay hangs while playing and recording at the same time in compat mode
4393819 SUNW,Sun-Blade-1000 panics with kernel heap corruption
4393967 WARNING: interrupt level 9 not serviced and audio hangs on Ultra 2
4400665 fix warlock problems in audio mixer
4402755 audio mixer should have save function to match restore function
4404373 Need driver fix for audio panic on BNlite systems
4404398 Birdsnestlite system require audio playback support from cdrom driver
4404559 SUNWauddx's depend file describes SUNWaudd as "Core Solaris Libraries"
4408726 am_attach() destroys mutex incorrectly
4411451 assertion, stpptr->am_ad_in & AM_APM_IN_DRIVER in am_ad.c
4412128 memory leak in am_close_audio
4415430 audio framework needs some small changes to improve header files
4416096 volume and balance broken in compatibility mode using audioplay
4418923 minor problems with play only and record only audio hardware
4417092 assertion precision != AUDIO_PRECISION_16    encoding .. in am_ad.c
4417298 audioplay does not play sequential files correctly in mixer mode
4423482 EOF count gets cleared when turning the mixer off
 
(from 113422-01)
 
4735539 enchilada server is not hotplug-aware on USB

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
       example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
       example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Reboot the system after patch installation.
 
	NOTE 1:	To get the full support for logical device namespace for
                printers and new printer minor node type, one needs to
                install the following patches:
 
		108529-03 (or newer)    kernel update patch
		108980-05 (or newer)    devfsadm patch
		109884-01 (or newer)    ecppsys.h patch
		109895-01 (or newer)    lp driver patch
		109878-01 (or newer)    dma_i8237A.h patch
		109891-01 (or newer)    pmserver.jar patch
		109897-01 (or newer)    USB patch
 
	NOTE 2: To get the full USB audio support for Solaris 8, one
                needs to install the following patches:
 
                108529-11 (or newer)    kernel update patch
                109897-06 (or newer)    USB Audio Patch
		111015-02 (or newer)    /platform/i86pc/kernel/drv/sbpro patch
 
		and these new packages from Solaris 8 Update 6 (10/01) Release:
 
		SUNWauda  (Solaris Audio Applications)
                SUNWuaud  (USB Audio Device Drivers)
                SUNWuaudh (Solaris header files for USB audio drivers
                                and applications)
 
	NOTE 3: To get the complete fix for bugid # 5028398, please install
		the following patch:
 
		116976-01 (or newer)    kadb patch

README -- Last modified date:  Tuesday, August 24, 2004

